     SINEX -   Solution (Software/technique) INdependent EXchange Format 

                        Version 2.00 (May 24, 2002)

 INTRODUCTION

The SINEX acronym was suggested by Blewitt et al. (1994) and the first versions, 0.04, 0.05, 1.00 evolved from the work and contributions of the SINEX Working Group of the IGS. The IGS Analysis Centres and Associated Analysis Centres use the SINEX format for their weekly solutions since mid 1995. Although the SINEX format was developped by the IGS, the ILRS and IVS decided to use it for their pilot projects as well because SINEX was designed to be modular and general enough to handle GPS as well as other techniques. To meet all the requirements for SLR and VLBI solutions some new elements and more detailed specifications were added by the ILRS Analysis Working Group and by the IVS. These extensions were merged with the previous SINEX version 1.00 to get a unique format definition for all space geodetic techniques, and after an intensive discussion the new version called SINEX 2.00 could be finalized. We have to thank the IGS Reference Frame Working Group chaired by R. Ferland, the ILRS Analysis Coordinator R. Noomen and the ILRS Analysis Working Group, the IVS Analysis Coordinator A. Nothnagel and Z. Altamimi from the ITRF section of IGN for their contributions and advice concerning a new SINEX format definition.
The changes from version 1.00 to 2.00 are given in the next section of this document. The complete and detailed format definition can be seen in APPENDIX I, and the relevant least squares adjustment formulas with their relations to the SINEX format are summarized in APPENDIX II.
 CHANGES FROM VERSION 1.00 TO 2.00

1) The version number in the header line changes to 2.00.

2) The list of allowed estimated parameter types has increased. As additional         parameters you can include in your solution: 

- XGC    \

- YGC    -  = coordinates of the geocenter [m]

- ZGC    /

- RS_RA     = right ascension of a radio source [rad]

- RS_DE     = declination of a radio source [rad]

- RS_RAR    = rate of right ascension of a radio source [rad/y]

- RS_DER    = rate of declination of a radio source [rad/y]

- RS_PL     = radio source parallax [rad]

- NUT_LN    = nutation total in longitude [rad]

- NUT_OB    = nutation total in obliquity [rad]

- NUTRLN    = nutation rate in longitude [rad/d]

- NUTROB    = nutation rate in obliquity [rad/d]

- TGNWET    = troposphere gradient in north for the wet part [m]  

- TGNDRY    = troposphere gradient in north for the dry part [m]

- TGNTOT    = total troposphere gradient in north (wet + dry part) [m]

- TGEWET    = troposphere gradient in east for the wet part [m]

- TGEDRY    = troposphere gradient in east for the dry part [m]

- TGETOT    = total troposphere gradient in east (wet + dry part) [m]

- AXI_OF    = antenna axis offset [m]

- RBIAS     = range bias [m]

- TBIAS     = time bias [ms]

- SBIAS     = scale bias [ppb]

- ZBIAS     = troposphere bias in zenith [m]

 The parameters LODR and UTR (LOD and UT1-UTC reduced for the short periodic terms up to 35 days) are no official SINEX parameters and should not be used.

 The coordinates of geocenter already appear in some IGS solutions, so we decided to define these parameters as officially allowed.

 The coordinates of radio sources (right ascension, declination) and their rates, the parallax of radio sources, the nutation parameters and their rates, the troposphere gradients and the antenna axis offsets are new parameters requested for VLBI solutions.

 The four bias parameters are taken from the ILRS implementation of SINEX.

3) Due to these new parameters the field 'Solution Contents' in the HEADER LINE     and in the block INPUT/HISTORY must be changed.

 All parameters belonging to the stations are summarized in only one character:

'S' = station coordinates (STAX, STAY, STAZ), 

      station velocities (VELX, VELY, VELZ), 

      all four bias parameters (RBIAS, TBIAS, SBIAS, ZBIAS),

      geocenter coordinates (XGC, YGC, ZGC).

That means, the character 'X' for station coordinates and 'V' for station velocities are dropped.

 A new character is defined for all parameters belonging to the celestial reference frame:

'C' = right ascension and declination of the radio sources (RS_RA, RS_DE),

      rates for right ascension and declination of the radio sources

      (RS_RAR, RS_DER),

      parallax of radio sources (RS_PL).

 The other new parameters can be attached easily to the existing characters of SINEX version 1.00:

'T' = for all troposphere parameters (including the new parameters for the 

      troposphere gradients TGNWET, TGNDRY, TGNTOT, TGEWET, TGEDRY, TGETOT),

'E' = for all earth orientation parameters (including the new nutation

      parameters NUT_LN, NUT_OB, NUTRLN, NUTROB).

 The orbit parameters 'O' are not changed.

4) The block SOLUTION/STATISTICS is now RECOMMENDED if the requested values are available because for a further combination of solutions it is necessary to have the complete statistical information.

 The preference is given to the original values like 'NUMBER OF OBSERVATIONS' and 'NUMBER OF UNKNOWNS' instead of 'DEGREE OF FREEDOM'.

 The 'NUMBER OF OBSERVATIONS' should represent only the number of 'real'          observations.

 A new value became necessary if unconstrained normal equations are stored because the variance factor contains the constraints of the solution. Therefore the weighted square sum of the vector 'observed minus computed' should be given in the SOLUTION/STATISTICS block to become independent of the influence of the constraints on the variance factor: (o-c)‘ P (o-c), where (o-c) represents the vector 'observed minus computed' and P denotes the weigth matrix. This new value can be stored under the name

 WEIGHTED SQUARE SUM OF O-C

5) The list of allowed parameter types in the block SOLUTION/APRIORI is extended following some IGS solutions: if you apply inner constraints to your solution you can add the constrained transformation parameters to the SOLUTION/APRIORI block. 

That means for the particular fields of this block:

- Parameter Type:

TX, TY, TZ     for translation restrictions in x, y and z direction

RX, RY, RZ     for rotation restrictions around the x, y and z axis

SC             for scale restriction

TXR, TYR, TZR  for restrictions on the rates of the translation in x, y  and z 

RXR, RYR, RZR  for restrictions on the rates of the rotation around the

               x, y and z axis

SCR            for restriction on the rate of the scale

- The fields Site Code, Point Code, Solution ID are filled with '-'

- Time:

the reference epoch of the inner constraints

- Parameter Units:

 m     for translation parameters, i.e. [m]

 mas   for rotation parameters, i.e. [mas]

 ppb   for the scale, i.e. [ppb]

 m/y   for the rates of translation parameters, i.e. [m/y]

 ma/y  for the rates of rotation parameters, i.e. [mas/y]

 pb/y  for the rate of the scale, i.e. [ppb/y]

- Constraint Code:

0 for tight constraints

- Parameter Apriori:

the value on which you constrained the transformation parameter or its rate for the transformation of your solution according to the apriori reference frame

(e.g. if the apriori reference frame represents the desired reference frame for your solution the apriori parameters are 0.0)

- Parameter Standard Deviation:

the sigma you choose for constraining the particular transformation parameter or its rate

To decide which stations were contributing to the inner constraints, the appropriate station parameters (coordinates and velocities if the rates are given as well) must be given in the block SOLUTION/APRIORI as well and should contain a '1' in the field 'CONSTRAINT CODE'.

6) With the new SINEX version the delivery of normal equations will be defined more precisely. We have now three possibilities include normal equation systems in the SINEX file:

a) In principle it was already possible in version 1.00 to store normal equation matrices in the two SOLUTION/MATRIX blocks (ESTIMATE and APRIORI) if you use matrix type INFO. And together with the two vectors in SOLUTION/ESTIMATE and SOLUTION/APRIORI you are able to reconstruct the original (reduced) normal equation system without constraints. But this procedure of removal the constraints and compute the right hand side of the normal equation system is always a little bit critical, and in addition to that problem, the procedure depends on the solution vector given in SOLUTION/ESTIMATE.

For a further combination of several solutions there would be less problems if the original normal equation system without any constraints can be stored directly in the SINEX file. In that case you have the advantage that the constraints applied in the individual solutions (SOLUTION/MATRIX_APRIORI) and the resulting solution vector (SOLUTION/ESTIMATE) have no influence on the combination. These considerations led to two other possibilities of storing normal equations in the SINEX file, but for both we had to introduce two new blocks for the original normal equation system:

- SOLUTION/NORMAL_EQUATION_VECTOR

This block contains the vector of the right hand side of the reduced normal  equation system

b = A' P l

  where 

  A'  is the transposed of the Jacobi-Matrix, 

  P   is the weight matrix of the observations and 

  l   is the vector observed minus computed with apriori values.

- SOLUTION/NORMAL_EQUATION_MATRIX

This block contains the reduced normal equation matrix WITHOUT constraints (i.e. the 'free' / original solution):

N = A‘ P A

The structure of this block is similar to the other two MATRIX blocks.

The indices of both new blocks must be consistent with the indices in SOLUTION/ESTIMATE.

With these two additional blocks the second and third possibility of storing normal equations look as follows:

b) You store the complete information about your solution in the following blocks:

- original normal equation matrix N = A‘ P A : SOLUTION/NORMAL_EQUATION_MATRIX

- vector of right hand side of original normal equation b = A‘ P l :

  SOLUTION/NORMAL_EQUATION_VECTOR

- apriori values of the unknown parameters x0: SOLUTION/APRIORI

- normal equation matrix of applied constraints in your solution dN:

  SOLUTION/MATRIX_APRIORI

- resulting unknown parameters of the constrained solution 


x = x0 + inv(N + dN) b : SOLUTION/ESTIMATE

The advantage of this method is the availability of the whole information, i.e. the original normal equation can be used for a further combination without any problems of constraints removal like in method a), and other users who are interested in the parameters of the constrained solution itself can take the vector in SOLUTION/ESTIMATE. 

A problem might occur when generating such a SINEX file because you need both, the original normal equation system as well as the solution estimate (as in case a)) and in most software packages the normal equation matrix might already be inverted at the time when you have the solution estimate available.

c) The third possibility is storing only the original normal equation system in the SINEX file, i.e.

- original normal equation matrix N = A‘ P A : SOLUTION/NORMAL_EQUATION_MATRIX

- vector of right hand side of original normal equation b = A‘ P l :

  SOLUTION/NORMAL_EQUATION_VECTOR

- apriori values of the unknown parameters x0: SOLUTION/APRIORI

For a further combination with other solutions this would be enough information and there wouldn’t be any problems with constraints removal.

On the other hand the documentation of the estimated parameters is missing.

To reconstruct the statistical information about the original solution for the last two possibilities (points b) and c)) it is necessary to store the weighted square sum of the vector observed minus computed, i.e.  l‘ P l in the SOLUTION/STATISTICS block because only this part of the variance factor is independent of the constrained solution and can be taken for a combination 

( v’ P v = l’ P l – (x – x0)‘ b ):

WEIGHTED SQUARE SUM OF O-C 

(see as well point 4) of the changes from version 1.00 to 2.00)

7) For more clearness and with regards to a good documentation how the solution in SOLUTION/ESTIMATE was created, the block SOLUTION/APRIORI is now mandatory.

The block SOLUTION/MATRIX_APRIORI is only mandatory if the matrix in SOLUTION/MATRIX_ESTIMATE contains some constraints.

 If you deliver normal equations in your SINEX file some more blocks are mandatory, depending on the method of storing normal equations: 

For method 6a)

- SOLUTION/MATRIX_APRIORI (INFO type)

- SOLUTION/MATRIX_ESTIMATE (INFO type)

- SOLUTION/STATISTICS (#observations, #unknowns, weighted square sum of o-c)

For method 6b)

- SOLUTION/MATRIX_APRIORI 

- SOLUTION/NORMAL_EQUATION_MATRIX

- SOLUTION/NORMAL_EQUATION_VECTOR

- SOLUTION/STATISTICS (#observations, #unknowns, weighted square sum of o-c)

For method 6c)

- SOLUTION/NORMAL_EQUATION_MATRIX

- SOLUTION/NORMAL_EQUATION_VECTOR

- SOLUTION/STATISTICS (#observations, #unknowns, weighted square sum of o-c)

8) Besides the new blocks for normal equations we have introduced some other     new blocks in the SINEX format 2.00:

- NUTATION/DATA: 

to store the information about the nutation model used in the analysis;

This block contains two fields: one for the name of the nutation model and one   for some comments.

- PRECESSION/DATA:

to store the information about the precession model used in the analysis;

This block contains two fields: one for the name of the precession model and     one for some comments.

- SOURCE/ID:

to provide information about the radio sources observed with VLBI;

There are 3 fields for source names: the Source Code (used for SINEX internal referencing), the IERS designation and the ICRF designation.

- BIAS/EPOCHS:

important if bias parameters are included in the solution (from SLR solutions)

9) The matrix type SRIF (for Square Root Information Filter Matrix) in the two blocks SOLUTION/MATRIX_APRIORI and SOLUTION/MATRIX_ESTIMATE is no longer allowed.

10) The longitude sign definition in the SITE/ID block is redefined according to the ISO6709 definition (that is the way the information was already stored in most of the SINEX files):

- positive longitudes have to be used for east direction with respect to the Greenwich meridian

- following the ISO6709 specification, the range of longitude should be 

[-180° +180°[

11) The value "-----" in the field 'Antenna Serial Number' of the SITE/GPS_PHASE_CENTER block is redefined:

it signifies that the phase center offsets for L1 and L2 that are given in the following columns apply to ALL antennas of the same type that is indicated in the field 'Antenna Type'. 

As a consequence, if the phase center offsets for one antenna name and the given model are the same for all antenna serial numbers, it is enough to store only one data line (with "-----" for the 'Antenna Serial Number') in the SITE/GPS_PHASE_CENTER block for each antenna type that appears in the SITE/ANTENNA block.

SINEX SYNTAX

SINEX is an ASCII file with lines of 80chars or less. It consists  of a

number of blocks which are mutually referenced (related) through station

codes/names, epochs and/or index counters. Some blocks consist of

descriptive lines (starting in Col.2) and/or fixed format fields with

numerous headers and descriptive annotations. 

The first line is MANDATORY and must start with "%" in col 1, and contains information about the  agency, file identification, solution spans, techniques, type of solution, etc. (for more details see the Appendix I or II). The last line ends with "%ENDSNX". 

The SINEX format consists of a number BLOCKS  which start with "+" in the

first col. followed by a standardized block labels, and each block ends

with "-" and the block label. Each block data starts in the column 2 or

higher. Blocks can be in any order, provided that they start with (+) and end with (-) block labels. The first header line and most blocks are

related through epochs or time stamps in the following format:

YY:DOY:SECOD  YY-year; DOY- day of year; SECOD -sec of day;

E.g. the epoch 95:120:86399  denotes April 30, 1995 (23:59:59UT). The

epochs  00:00:00000 are allowed in all blocks (except the first header

line) and default into the start or end epochs of the first header line

which must always be coded. This is particularly useful for some blocks,

such as the ones related to hardware, occupancy, which should be centrally archived by IGSCB with 00:00:00000 as the end (current) epochs, and which should be readily usable by ACs for SINEX and other analysis/processing as official (authoritative) IGS information.
COMMENT lines starts with "*" in Col. 1 and can be anywhere within or

outside a block, though for the clarity sake, beginning and ends of blocks are preferable. For increased portability, the floating number exponent of "E" should be used rather than "D" or "d" which is not recognized by some compiler/installations. Fields not coded should be filled with "-" characters to allow efficient row and column format readings.

The most important blocks are the SOLUTION blocks. They are in fixed format (For more information on the format, see APPENDIX I). 

The mandatory SOLUTION blocks depend on the contents of the SINEX file.

If you deliver variance-covariance matrices or correlation matrices in your SINEX files the blocks

- SOLUTION/ESTIMATE

- SOLUTION/APRIORI

- SOLUTION/MATRIX_ESTIMATE

are mandatory. 

The block SOLUTION/MATRIX_APRIORI is only mandatory if the matrix in SOLUTION/MATRIX_ESTIMATE contains some constraints. 

Important but not mandatory (though STRONGLY RECOMMENDED if available for IERS purposes) is the block SOLUTION/STATISTICS, especially the information about the number of observations, the number of unknowns and the variance factor.

 If you deliver normal equations in your SINEX file the mandatory SOLUTION blocks depend on the method of storing normal equations: 

For method 6a)

- SOLUTION/APRIORI

- SOLUTION/ESTIMATE

- SOLUTION/MATRIX_APRIORI (INFO type)

- SOLUTION/MATRIX_ESTIMATE (INFO type)

- SOLUTION/STATISTICS (#observations, #unknowns, weighted square sum of o-c)

For method 6b)

- SOLUTION/APRIORI

- SOLUTION/ESTIMATE

- SOLUTION/MATRIX_APRIORI 

- SOLUTION/NORMAL_EQUATION_MATRIX

- SOLUTION/NORMAL_EQUATION_VECTOR

- SOLUTION/STATISTICS (#observations, #unknowns, weighted square sum of o-c)

For method 6c)

- SOLUTION/APRIORI

- SOLUTION/NORMAL_EQUATION_MATRIX

- SOLUTION/NORMAL_EQUATION_VECTOR

- SOLUTION/STATISTICS (#observations, #unknowns, weighted square sum of o-c)

Storing the (reduced) normal equation system in one of the possible ways described before is encouraged for combination research purposes within the IERS to avoid the critical step of constraints removal.

The scale of estimated and apriori standard deviations can, in principle, be arbitrary (note even apriori scaling is arbitrary, depending on the observation weighting). However, both estimated and apriori standard deviations (and the corresponding matrices) MUST use the same scaling (i.e. variance) factor stored in the block SOLUTION/STATISTICS. Otherwise the apriori information cannot be  rigorously removed to form free solutions (e.g. normal matrices). Scaling between different SINEX solutions is beyond the SINEX format and must be dealt with at the combination/analysis stage.
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1. Introduction

This document describes the Software Independent Exchange (SINEX) format. It started in early 1995 with an effort by a number of IGS participants and it was designed to be easily extended. For the new IERS structure, operational since January 1, 2001, and due to the use of SINEX by the ILRS (pilot project 'positioning and earth orientation') and the IVS as well, some extensions were made with the purpose to have a unique format description for all techniques.

2. Data Structure

Each SINEX line has at most 80 ASCII characters.

The SINEX file is subdivided in groups of data called blocks. Each block is 

enclosed by a header and trailer line. Each block has a fixed format. The 

blocks contain information on the file, its input, the sites and the solution. 

All elements within a line are defined. A character field without information will have "-"s within its field and a missing numerical element will have a value of 0 within its field. Therefore the SINEX file is accessible "column-wise" as well as "line-wise". Character fields should be left hand justified whenever applicable.

 The first character of each line identify the type of information that the 

line contains. Five characters are reserved. They have the following 

meaning when they are at the beginning of a line, they identify:

 Character
Definition

 "%"            Header and trailer line,

 "*"            Comment line within the header and trailer line,

 "+"            Title at the start of a block

 "-"            Title at the end of a block

 " "            Data line within a block

 No other character is allowed at the beginning of a line!

 A SINEX file must start with a header line and ends with a footer line.

 The following blocks are defined:

 FILE/REFERENCE

 FILE/COMMENT

 INPUT/HISTORY

 INPUT/FILES

 INPUT/ACKNOWLEDGEMENTS

 NUTATION/DATA

 PRECESSION/DATA

 SOURCE/ID

 SITE/ID

 SITE/DATA

 SITE/RECEIVER

 SITE/ANTENNA

 SITE/GPS_PHASE_CENTER

 SITE/ECCENTRICITY

 BIAS/EPOCHS

 SOLUTION/EPOCHS
 SOLUTION/STATISTICS

 SOLUTION/ESTIMATE

 SOLUTION/APRIORI

 SOLUTION/MATRIX_ESTIMATE {p} {type}

 SOLUTION/MATRIX_APRIORI {p} {type}

 SOLUTION/NORMAL_EQUATION_VECTOR  

 SOLUTION/NORMAL_EQUATION_MATRIX {p}


Where:
{p}     L or U


      
{type}  CORR or COVA or INFO

These block titles are immediately preceded by a "+" or a "-" as 

they mark the beginning or the end of a block. The block titles  must be in

capital letters. After a block has started(+) it must be ended(-) before another

block can begin. The general structure is as follow:

%=SNX........... (Header line)----------|

.............                           |

+(BLOCK TITLE)-------------|            |

 ............              |            |

 ............              |            |

 ............              |            |

-(BLOCK TITLE)-------------|            |

.............                           |

+(BLOCK TITLE)-------------|            |

 ............              |            |

 ............              |            |

 ............              |            |

-(BLOCK TITLE)------------ |            |

.............                           |

%ENDSNX          (Trailer line)---------|

Most fields within a SINEX line are separated by a single space. In the 

following sections, each SINEX line is defined by its field name, a general 

description and the (FORTRAN) format.

A comment line (not to be confused with the FILE/COMMENT Block) can be written anywhere within the header and the footer line. All comment lines must start with a "*" in the first column. With the use of this character information can be hidden from the software reading the file without deleting it from the file. A comment line is defined as follow:


 ___________________________________________________________________


|______________________C_O_M_M_E_N_T___D_A_T_A___L_I_N_E____________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Comment        | Any general comment relevant to   |   1H*,A79    |


|                | the SINEX file.                   |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |      80      |

                                                           |______________|

 Some fields are found in several blocks. To keep the description short, they are described in detail here, and will be referred to in the sections with additional information added when necessary. The fields defined below will be referenced to by putting them within square brackets [] when encountered in the following sections.


 ____________________________________________________________________


|                |                                    |              |


|__Field_________|______Description___________________|___Format_____|


|                |                                    |              |


| Time           | YY:DDD:SSSSS.  "UTC"               |   I2.2,      |


|                | YY = last 2 digits of the year,    |   1H:,I3.3,  |


|                | if YY <= 50 implies 21-st century, |   1H:,I5.5   |


|                | if YY > 50 implies 20-th century,  |              |


|                | DDD = 3-digit day in year,         |              |


|                | SSSSS = 5-digit seconds in day.    |              |


|________________|____________________________________|______________|


|                |                                    |              |


| Constraint Code| Single digit indicating the        |   A1         |


|                | constraints:                       |              |


|                | 0-fixed/tight constraints,         |              |


|                | 1-significant constraints,         |              |


|                | 2-unconstrained.                   |              |


|________________|____________________________________|______________|


|                |                                    |              |


| Parameter Type | Type of parameter.                 |   A6         |


|                | List of allowed parameters and the |              |

      |                | units provided:                    |              |


|                |                                    |              |


|                | STAX   - station X coordinate,    m|              |


|                | STAY   - station Y coordinate,    m|              |


|                | STAZ   - station Z coordinate,    m|              |


|                | VELX   - station X velocity,    m/y|              |


|                | VELY   - station Y velocity,    m/y|              |


|                | VELZ   - station Z velocity,    m/y|              |

      |                | XGC    - geocenter X coordinate,  m|              |

      |                | YGC    - geocenter Y coordinate,  m|              |

      |                | ZGC    - geocenter Z coordinate,  m|              |

      |                | RS_RA  - radio source right        |              |

      |                |          ascension,             rad|              |

      |                | RS_DE  - radio source declin.,  rad|              |

      |                | RS_RAR - radio source right        |              |

      |                |          ascension rate,      rad/y|              |

      |                | RS_DER - radio source              |              |

      |                |          declination rate,    rad/y|              |

      |                | RS_PL  - radio source parallax, rad|              |


|                | LOD    - length of day,          ms|              |


|                | UT     - delta time UT1-UTC,     ms|              |

 
|                | XPO    - X polar motion,        mas|              |


|                | YPO    - Y polar motion,        mas|              |


|                | XPOR   - X polar motion rate, mas/d|              |


|                | YPOR   - Y polar motion rate, mas/d|              |

      |                | NUT_LN – total nutation in         |              |

      |                |          longitude,             rad|              |

      |                | NUT_OB – total nutation in         |              |

      |                |          obliquity,             rad|              |

      |                | NUTRLN - nutation rate in          |              |

      |                |          longitude,           rad/d|              |

      |                | NUTROB - nutation rate in          |              |

      |                |          obliquity            rad/d|              |

      |                | SAT__X - Satellite X coord.,      m|              |

      |                | SAT__Y - Satellite Y coord.,      m|              |

      |                | SAT__Z - Satellite Z coord.,      m|              |

      |                | SAT_VX - Satellite X velocity,  m/s|              |

      |                | SAT_VY - Satellite Y velocity,  m/s|              |

      |                | SAT_VZ - Satellite Z velocity,  m/s|              |

      |                | SAT_RP - Radiation pressure,       |              |

      |                | SAT_GX - GX scale,                 |              |

      |                | SAT_GZ - GZ scale,                 |              |

      |                | SATYBI - GY bias,              m/s2|              |

      |                | TROTOT - wet + dry Tropo delay,   m|              |

      |                | TRODRY - dry Tropo delay,         m|              |

      |                | TROWET - wet Tropo delay,         m|              |

      |                | TGNTOT – troposphere gradient      |              |

      |                |          in north (wet + dry),    m|              |

      |                | TGNWET – troposphere gradient      |              |

      |                |          in north (only wet),     m|              |

      |                | TGNDRY – troposphere gradient      |              |

      |                |          in north (only dry),     m|              |

      |                | TGETOT - troposphere gradient      |              |

      |                |          in east (wet + dry),     m|              |

      |                | TGEWET – troposphere gradient      |              |

      |                |          in east (only wet),      m|              |

      |                | TGEDRY – troposphere gradient      |              |

      |                |          in east (only dry),      m|              |

      |                | RBIAS  - range bias,              m|              |

      |                | TBIAS  - time bias,              ms|              |

      |                | SBIAS  - scale bias,            ppb|              |

      |                | ZBIAS  - troposphere bias at       |              |

      |                |          zenith,                  m|              |

      |                | AXI_OF - antenna axis offset,     m|              |


|________________|____________________________________|______________|


|                |                                    |              |


| Site Code      | - For stations:                    |   A4         |


|                | Call sign for a site.(It should be |              |


|                | consistent with ITRF, see below).  |              |

      |                | - For satellites:                  |              |

      |                | Use "PRXX" where XX is the PRN     |              |

      |                | number.                            |              |


|________________|____________________________________|______________|


|                |                                    |              |

      | Point Code     | - For stations:                    |   A2         |


|                | A two character code identifying   |              |


|                | physical monument within a site.   |              |


|                | Typically has a code A, but could  |              |


|                | vary if the site has more than one |              |


|                | monument.                          |              |

      |                | - For bias parameters: satellite ID|              |

      |                | L1, L2 for LAGEOS-1 or -2;         |              |

      |                | LC for combined LAGEOS;            |              |

      |                | E1, E2 for Etalon 1 or 2;          |              |

      |                | EC for combined Etalon;            |              |


|________________|____________________________________|______________|


|                |                                    |              |


| Solution ID    | Character identifying the solution |   A4         |


|                | given for a point at a site.       |              |

      |                | "----" applies to all.             |              |


|________________|____________________________________|______________|


|                |                                    |              |


| Observation    | A single character indicating the  |   A1         |


| Code.          | technique(s) used to arrive at the |              |


|                | solutions obtained in this SINEX   |              |


|                | file. It should be consistent with |              |


|                | the IERS convention.               |              |


|                | This character code may be:        |              |


|                | C-Combined techniques used.        |              |


|                | D-DORIS,                           |              |


|                | L-SLR,                             |              |


|                | M-LLR,                             |              |


|                | P-GPS,                             |              |


|                | R-VLBI.                            |              |


|________________|____________________________________|______________|

 Comment:

 For the official IERS sites the values of the 'Site Code' are listed in

ftp://lareg.ensg.ign.fr/pub/itrf/iers_dir.sta

 'Per year' means 365.25 days in this context.

3. Header Line (Mandatory)

  Description

 The header line must be the first line in a SINEX file.

  Contents:


 ___________________________________________________________________


|_____________H_E_A_D_E_R___L_I_N_E_________________________________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| First Character| Single character '%' in column #1.|   A1         |


|                | No other character than '%' is al-|              |


|                | lowed.                            |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Second         | Single character '=' in column #2.|   A1         |


| Character      | Indicates 'resultant' solution.   |              |


|                | No other character than '=' is al-|              |


|                | lowed.                            |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Document Type  | Three characters 'SNX' in columns |   A3         |


|                | 3 to 5. Indicates that this is a  |              |


|                | SINEX document.                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Format Version | Four digits indicating the version|   1X,F4.2    |


|                | of SINEX format used.             |              |


|                | '2.00' for this version.          |              |


|________________|___________________________________|______________|


|                |                                   |              |


| File Agency    | Identify the agency creating the  |   1X,A3      |


| Code           | file.                             |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Creation time of this SINEX file. |   1X,I2.2,   |


|                |                                   |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Agency Code]  | Identify the agency providing the |   1X,A3      |


|                | data in the SINEX file            |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Start time of the data used in the|   1X,I2.2,   |


|                | SINEX solution                    |   1H:,I3.3,  |


|                | Value 00:000:00000 should be      |   1H:,I5.5   |


|                | avoided.                          |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | End time of the data used in the  |   1X,I2.2,   |


|                | SINEX solution                    |   1H:,I3.3,  |


|                | Value 00:000:00000 should be      |   1H:,I5.5   |


|                | avoided.                          |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Observation   | Technique(s) used to generate the |   1X,A1      |


| Code]          | SINEX solution                    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Number of Est- | Number of parameters estimated in |   1X,I5.5    |


| timates        | this SINEX file.                  |              |


|                | Mandatory field.                  |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Constraint    | Single character indicating the   |   1X,A1      |


| Code]          | constraint in the SINEX solution. |              |


|                | Mandatory field.                  |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Solution       | Solution types contained in this  |   5(1X,A1)   |


| Contents       | SINEX file. Each character in this|              |


|                | field may be one of the following:|              |


|                |    S – all station parameters,    |              |

      |                |        i.e. station coordinates,  |              |

      |                |        station velocities, biases,|              |

      |                |        geocenter,                 |              |


|                |    O - Orbits,                    |              |


|                |    E - Earth Orientation Parameter|              |


|                |    T – Troposphere,               |              |

      |                |    C – Celestial Reference Frame  |              |


|                |    BLANK                          |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     77       |

                                                           |______________|

 Relationship with other blocks:

 This line is duplicated as the resultant line of the INPUT/HISTORY block with

the exception of its first character.

4. FILE/REFERENCE Block (Mandatory)

  Description:

  This block provides information on the Organization, point of contact, the

  software and hardware involved in the creation of the file.

  Contents:

 
 ___________________________________________________________________


|__________F_I_L_E___R_E_F_E_R_E_N_C_E___D_A_T_A___L_I_N_E__________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Information    | Describes the type of information |   1X,A18     |


| Type           | present in the next field. May    |              |


|                | take on the following values:     |              |


|                |                                   |              |


|                | 'DESCRIPTION' - Organization(s)   |              |


|                |                 gathering/altering|              |


|                |                 the file contents.|              |


|                | 'OUTPUT'      - Description of the|              |


|                |                 file contents.    |              |


|                | 'CONTACT'     - Address of the    |              |


|                |                 relevant contact. |              |

      |                |                 e-mail            |              |


|                | 'SOFTWARE'    - Software used to  |              |


|                |                 generate the file.|              |


|                | 'HARDWARE'    - Computer hardware |              |


|                |                 on which above    |              |


|                |                 software was run. |              |


|                | 'INPUT'       - Brief description |              |


|                |                 of the input used |              |


|                |                 to generate this  |              |


|                |                 solution.         |              |


|                |                                   |              |


|                | Any of the above fields may be    |              |


|                | and in any order.                 |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Information    | Relevant information for the type |   1X,A60     |


|                | indicated by the previous field.  |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

5. FILE/COMMENT Block (Optional)

 Description:

 This block can be used to provide general comments about the SINEX data file.

 Contents:

 
 ___________________________________________________________________


|____________F_I_L_E___C_O_M_M_E_N_T___D_A_T_A___L_I_N_E____________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Comment        | Any general comment providing     |   1X,A79     |


|                | relevant information about the    |              |


|                | SINEX file.                       |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

6. INPUT/HISTORY Block (Recommended)

 Description:

 This block provides information about the source of the information used to 

create the current SINEX file.

 Contents:


 ___________________________________________________________________


|__________I_N_P_U_T___H_I_S_T_O_R_Y___D_A_T_A___L_I_N_E____________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| File Code      | Only one of the following charac- |   1X,A1      |


|                | ters is permitted:                |              |


|                |    '+' - This character indicates |              |


|                |          that the information that|              |


|                |          follows identify an input|              |


|                |          solution contributing to |              |


|                |          this SINEX file.         |              |


|                |    '=' - This character indicates |              |


|                |          that the information that|              |


|                |          follows identify the     |              |


|                |          output solution file.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Document Type  | Three characters 'SNX' in columns |   A3         |


|                | 3 to 5. Indicates that this is a  |              |


|                | SINEX document.                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Format Version | Four digits indicating the version|   1X,F4.2    |


|                | of SINEX format used.             |              |


|                | '2.00' for this version.          |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Agency Code]  | Identify the agency creating the  |   1X,A3      |


|                | file.                             |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Creation time of this SINEX file. |   1X,I2.2,   |


|                |                                   |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Agency Code]  | Identify the agency providing the |   1X,A3      |


|                | data in the SINEX file.           |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Start time of the data used in the|   1X,I2.2,   |


|                | SINEX solution.                   |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | End time of the data used in the  |   1X,I2.2,   |


|                | SINEX solution.                   |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Observation   | Technique(s) used to generate the |   1X,A1      |


| Technique]     | SINEX solution.                   |              |


|                |                                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Number of Est- | Number of parameters estimated in |   1X,I5.5    |


| timates        | this SINEX file.                  |              |


|                |                                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Constraint    | Single digit indicating the       |   1X,A1      |


| Code]          | constraint in the SINEX solution. |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Solution       | Solution types contained in this  |   5(1X,A1)   |


| Contents       | SINEX file. Each character in this|              |


|                | field may be one of the following:|              |


|                |    S – all station parameters,    |              |

      |                |        i.e. station coordinates,  |              |

      |                |        station velocities, biases,|              |

      |                |        geocenter,                 |              |


|                |    O - Orbits,                    |              |


|                |    E - Earth Orientation Parameter|              |

      |                |    T – Troposphere,               |              |

      |                |    C – Celestial Reference Frame  |              |


|                |    BLANK                          |              |


|                |                                   |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     77       |

                                                           |______________|

 Comment:

 The final data line "=" describes the current SINEX file and match the 

header line with the exception of the first character.

7. INPUT/FILES Block (Optional)

 Description:

 This block identify the input files (and the current SINEX file) and allow for a short comment to be added to describe those files.

 Contents:

 
 ___________________________________________________________________


|____________I_N_P_U_T___F_I_L_E_S___D_A_T_A___L_I_N_E______________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Agency   Code]| Agency creating the solution des- |   1X,A3      |


|                | cribed in this data line.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time of creation of the input     |   1X,I2.2,   |


|                | SINEX solution                    |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5,  |


|________________|___________________________________|______________|


|                |                                   |              |


| File Name      | Name of the file containing the   |   1X,A29     |


|                | solution described in the current |              |


|                | data line.                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| File           | General description of the file   |   1X,A32     |


| Description    | referred to on this data line.    |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

 Comments:

 There must be exactly one INPUT/FILES data line for every INPUT/HISTORY data

line. The final data line must describe this current SINEX file.

8. INPUT/ACKNOWLEDGEMENTS Block (Optional)

 Description:

 This block defines the agency codes contributing to the SINEX file.

 Contents:

 
 ___________________________________________________________________


|___I_N_P_U_T___A_C_K_N_O_W_L_E_D_G_M_E_N_T_S___D_A_T_A___L_I_N_E___|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Agency Code]  | Agency(ies) contributing to this  |   1X,A3      |


|                | SINEX file.                       |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Agency         | Description of agency code.       |   1X,A75     |


| Description    |                                   |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

9. NUTATION/DATA Block (Mandatory for VLBI)

 Description:

 This block contains the nutation model used in the analysis procedure.

 Contents:               


 ___________________________________________________________________


|_________________N_U_T_A_T_I_O_N___D_A_T_A___L_I_N_E_______________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |

      | Nutation Code  | Code for nutation reference:      |   1X,A8      |

      |                | IAU1980                           |              |

      |                | IERS1996                          |              |

      |                | IAU2000a                          |              |

      |                | IAU2000b                          |              |

      |________________|___________________________________|______________|

      |                |                                   |              |

      | Comments       | General description of the        |   1X,A70     |

      |                | nutation model used               |              |

      |________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

 COMMENT:

 It must be a generally accepted model which is accessible to all users.

10. PRECESSION/DATA Block (Mandatory for VLBI)

 Description:

 This block contains the precession model used in the analysis procedure.

 Contents:                       


 ___________________________________________________________________


|_______________P_R_E_C_E_S_S_I_O_N___D_A_T_A___L_I_N_E_____________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |

      | Precess. Code  | Code for precession reference:    |   1X,A8      |

      |                | IAU1976                           |              |

      |                | IERS1996                          |              |

      |________________|___________________________________|______________|

      |                |                                   |              |

      | Comments       | General description of the        |   1X,A70     |

      |                | nutation model used               |              |

      |________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

COMMENT:

 It must be a generally accepted model which is accessible to all users.

11. SOURCE/ID (Mandatory for VLBI)

 Description:

 This block contains information about the radio sources estimated in the analysis, especially the names used in ICRF and for IERS.

 Contents:                       


 ___________________________________________________________________


|_____________R_A_D_I_O___S_O_U_R_C_E___D_A_T_A___L_I_N_E___________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |

      | Source Code    | Call sign for a source            |   1X,A4      |

      |________________|___________________________________|______________|

      |                |                                   |              |

      | IERS des.      | IERS designation of the radio     |   1X,A8      |

      |                | source                            |              |

      |________________|___________________________________|______________|

      |                |                                   |              |

      | ICRF des.      | ICRF designation of the radio     |   1X,A16     |

      |                | source                            |              |

      |________________|___________________________________|______________|

      |                |                                   |              |

      | Comments       | Comments or other names of the    |   1X,A68     |

      |                | radio source                      |              |

      |________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

12. SITE/ID Block (Mandatory)

 Description:

 This block provides general information for each site containing estimated 

parameters.

 Contents:


 ___________________________________________________________________


|_________________S_I_T_E___I_D___D_A_T_A___L_I_N_E_________________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Site Code]    | Call sign for a site.             |   1X,A4      |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Physical monument used at a site  |   1X,A2      |


|________________|___________________________________|______________|


|                |                                   |              |

      | Unique Monument| Unique alpha-nummeric monument    |   1X,A9      |

      | Identification | identification. For ITRF purposes,|              |


|                | it is a nine character DOMES/DOMEX|              |


|                | number (five/six digits, followed |              |


|                | by  the single letter 'M' or 'S', |              |

      |                | followed by four/three digits)    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Observation   | Observation technique(s) used.    |   1X,A1      |


| Code]          |                                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Station        | Free-format description of the    |   1X,A22     |


| Description    | site, typically the town and/or   |              |


|                | country.                          |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Approximate    | Approximate longitude of the site |   1X,I3,     |


| Longitude      | in degrees(E/+), minutes and      |   1X,I2,     |


|                | seconds.                          |   1X,F4.1    |


|________________|___________________________________|______________|


|                |                                   |              |


| Approximate    | Approximate latitude of the site  |   1X,I3,     |


| Latitude       | in degrees(NS/+-), minutes and    |   1X,I2,     |


|                | seconds.                          |   1X,F4.1    |


|________________|___________________________________|______________|


|                |                                   |              |


| Approximate    | Approximate height of the site in |   1X,F7.1    |


| Height         | metres.                           |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     75       |

                                                           |______________|

 Comments:

 For DOMES numbers and station description as well as for Site Codes please refer to

  ftp://lareg.ensg.ign.fr/pub/itrf/iers_dir.sta 

 If a DOMES number is not available (e.g. for a new station), please ask Zuheir Altamimi for a DOMES number (altamimi@ensg.ign.fr).

 Use the minus sign for negative approximate longitude or latitude only in the "degrees" component and don't repeat it in the "minutes" and "seconds" component.

 Following the ISO6709 specification, the range of longitude should be [-180° +180°[.

13. SITE/DATA Block (Optional)

 Description:

 This block gives the relationship between the estimated station parameters 

in the SINEX file and in the input files.

 Contents: 


 ___________________________________________________________________


|_________S_I_T_E___D_A_T_A___L_I_N_E_______________________________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Site Code]    | Site Code for solved station      |   1X,A4      |


|                | coordinates.                      |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point Code for solved station     |   1X,A2      |


|                | coordinates.                      |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution number to which the input|   1X,A4      |


|                | in this data line is referred to. |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Site Code]    | Site Code from an input SINEX file|   1X,A4      |


|                |                                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point code from an input SINEX    |   1X,A2      |


|                | file.                             |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution Number for a Site/Point  |   1X,A4      |


|                | from an input SINEX file.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Observation   | Observation Code for a Site/Point/|   1X,A1      |


| Code]          | Solution Number from an input     |              |


|                | SINEX file.                       |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time of start of data for the     |   1X,I2.2,   |


|                | input SINEX file.                 |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time of end of data for the input |   1X,I2.2,   |


|                | SINEX file.                       |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Agency Code]  | Creation Agency Code for the input|   1X,A3      |


|                | SINEX file.                       |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Creation time for the input SINEX |   1X,I2.2,   |


|                | file.                             |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     71       |

                                                           |______________|

 Comment:

 Times must refer to observation epochs.

14. SITE/RECEIVER Block (Mandatory for GPS)

 Description:

 List the receiver used at each site during the observation period of 

interest.

 Contents:  


 ___________________________________________________________________


|_____S_I_T_E___R_E_C_E_I_V_E_R___D_A_T_A___L_I_N_E_________________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Site Code]    | Site code for which some          |   1X,A4      |


|                | parameters are estimated.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point Code at a site for which    |   1X,A2      |


|                | some parameters are estimated.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution Number at a Site/Point   |   1X,A4      |


|                | code for which some parameters    |              |


|                | are estimated.                    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Observation   | Identification of the observation |   1X,A1      |


| Code]          | technique used.                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time since the receiver has been  |   1X,I2.2,   |


|                | operating at the Site/Point.      |   1H:,I3.3,  |


|                | Value 00:000:00000 indicates that |   1H:,I5.5   |


|                | the receiver has been operating   |              |


|                | at least since the "File Epoch    |              |


|                | Start Time".                      |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time until the receiver is opera- |   1X,I2.2,   |


|                | ted at a Site/Point.              |   1H:,I3.3,  |


|                | Value 00:000:00000 indicates that |   1H:,I5.5   |


|                | the receiver has been operating   |              |


|                | at least until the "File Epoch    |              |


|                | End Time".                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Receiver Type  | Receiver Name & model.            |   1X,A20     |


|________________|___________________________________|______________|


|                |                                   |              |


| Receiver       | Serial number of the receiver.    |   1X,A5      |


| Serial Number  | Takes on value '-----' if unknown.|              |


|________________|___________________________________|______________|


|                |                                   |              |


| Receiver       | Firmware used by this receiver    |   1X,A11     |


| Firmware       | during the epoch specified above. |              |


|                | Takes on value '---------------'  |              |


|                | if unknown.                       |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

  Comments:

 - For IGS standard receiver names please refer to

   ftp://igscb.jpl.nasa.gov/igscb/station/general/rcvr_ant.tab

15. SITE/ANTENNA Block (Mandatory for GPS)

 Description:

 List of antennas used at each site used in the SINEX file.

 Contents:  


 ___________________________________________________________________


|_______S_I_T_E___A_N_T_E_N_N_A___D_A_T_A___L_I_N_E_________________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Site Code]    | Site code for which some          |   1X,A4      |


|                | parameters are estimated.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point Code at a site for which    |   1X,A2      |


|                | some parameters are estimated.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution Number at a Site/Point   |   1X,A4      |


|                | code for which some parameters    |              |


|                | are estimated.                    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Observation   | Identification of the observation |   1X,A1      |


| Code]          | technique used.                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time since the antenna  has been  |   1X,I2.2,   |


|                | installed at the Site/Point.      |   1H:,I3.3,  |


|                | Value 00:000:00000 indicates that |   1H:,I5.5   |


|                | the antenna has been installed    |              |


|                | at least since the "File Epoch    |              |


|                | Start Time".                      |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time until the antenna is instal- |   1X,I2.2,   |


|                | led at a Site/Point.              |   1H:,I3.3,  |


|                | Value 00:000:00000 indicates that |   1H:,I5.5   |


|                | the antenna has been installed    |              |


|                | at least until the "File Epoch    |              |


|                | End Time".                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Antenna Type   | Antenna name & model.             |   1X,A20     |


|________________|___________________________________|______________|


|                |                                   |              |


| Antenna        | Serial number of the antenna.     |   1X,A5      |


| Serial Number  | Takes on value '-----' if unknown.|              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     68       |

                                                           |______________|

Comments:

 - For IGS standard antenna names please refer to

   ftp://igscb.jpl.nasa.gov/igscb/station/general/rcvr_ant.tab

16. SITE/GPS_PHASE_CENTER Block (Mandatory for GPS)

 Description:

 List of GPS phase center offsets for the antennas described in the Site 

Antenna block. The offset is given from the Antenna Reference Point (ARP) to 

the L1 and L2 phase centers respectively. 

 Contents:

 
 ___________________________________________________________________


|_______G_P_S___P_H_A_S_E___C_E_N_T_E_R___D_A_T_A___L_I_N_E_________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Antenna Type   | Antenna name & model.             |   1X,A20     |


|________________|___________________________________|______________|


|                |                                   |              |


| Antenna        | Serial number of the antenna.     |   1X,A5      |


| Serial Number  | Takes on value '-----' if the     |              |


|                | phase center offsets apply to all |              |


|                | antennas of the same type.        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| L1 Phase Center| Up(+) offset from the ARP to      |   1X,F6.4    |


| Up Offset      | the L1 phase center in meters.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| L1 Phase Center| North(+) offset from the ARP to   |   1X,F6.4    |


| North Offset   | the L1 phase center in meters.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| L1 Phase Center| East(+) offset from the ARP to    |   1X,F6.4    |


| East Offset    | the L1 phase center in meters.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| L2 Phase Center| Up(+) offset from the ARP to      |   1X,F6.4    |


| Up Offset      | the L2 phase center in meters.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| L2 Phase Center| North(+) offset from the ARP to   |   1X,F6.4    |


| North Offset   | the L2 phase center in meters.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| L2 Phase Center| East(+) offset from the ARP to    |   1X,F6.4    |


| East Offset    | the L2 phase center in meters.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Antenna Cali-  | Name of the antenna model used in |   1X,A10     |


| bration model  | the correction of the observations|              |

      |                | for phase center variations.      |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

 Comments:

 For IGS purposes see the IGS Central Bureau Information System for ARPs and antenna phase center offsets:

 directory: igscb/station/general/

 files: antenna.gra and rcv_ant.tab   

 If the phase center offsets for one antenna type (antenna name and the given model) are the same for all antenna serial numbers, it is enough to store only one data line (with '-----' for the 'Antenna Serial Number') in this block for each antenna type that appears in the SITE/ANTENNA block.

17. SITE/ECCENTRICITY Block (Mandatory)

 Description:

 List of antenna eccentricities from the Marker to the Antenna Reference 

Point (ARP) or to the intersection of axis.

 Contents:


 ___________________________________________________________________


|__S_I_T_E____E_C_C_E_N_T_R_I_C_I_T_Y___D_A_T_A___L_I_N_E___________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Site Code]    | Site code for which some          |   1X,A4      |


|                | parameters are estimated.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point Code at a site for which    |   1X,A2      |


|                | some parameters are estimated.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution ID at a Site/Point       |   1X,A4      |


|                | code for which some parameters    |              |


|                | are estimated.                    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Observation   | Identification of the observation |   1X,A1      |


| Code]          | technique used.                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time since the antenna has been   |   1X,I2.2,   |


|                | installed at the Site/Point.      |   1H:,I3.3,  |


|                | Value 00:000:00000 indicates that |   1H:,I5.5   |


|                | the antenna has been installed    |              |


|                | at least since the "File Epoch    |              |


|                | Start Time".                      |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Time until the antenna is instal- |   1X,I2.2,   |


|                | led at a Site/Point.              |   1H:,I3.3,  |


|                | Value 00:000:00000 indicates that |   1H:,I5.5   |


|                | the antenna has been installed    |              |


|                | at least until the "File Epoch    |              |


|                | End Time".                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Eccentricity   | Reference system used to describe |   1X,A3      |


| Reference      | vector distance from monument     |              |


| System         | benchmark to the antenna reference|              |


|                | point or intersection of axis:    |              |


|                | 'UNE' - Local reference system    |              |


|                |         Up, North, East.          |              |


|                | 'XYZ' - Cartesian Reference System|              |


|                |         X, Y, Z.                  |              |


|                | All units are in meters.          |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Up / X         | Up / X  offset from the marker to |   1X,F8.4    |


| Eccentricity   | the Antenna reference point (ARP).|              |


|________________|___________________________________|______________|


|                |                                   |              |


| North / Y      | North/Y offset from the marker to |   1X,F8.4    |


| Eccentricity   | the Antenna reference point (ARP).|              |


|________________|___________________________________|______________|


|                |                                   |              |


| East / Z       | East/Z  offset from the marker to |   1X,F8.4    |


| Eccentricity   | the Antenna reference point (ARP).|              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     72       |

                                                           |______________|

  Comments:

 - At the moment the local ties used in the ITRF2000 primary combination are only 

   available throughout a login/password ftp access. To get access to these values  

   please contact Zuheir Altamimi (altamimi@ensg.ign.fr).

 - An older (March 23, 1999) listing of the official values for IERS sites is 

   available at

   ftp://lareg.ensg.ign.fr/pub/itrf/iers.ecc

 - For GPS (antenna heights) you can refer to the daily generated IGS SINEX template:

   ftp://igscb.jpl.nasa.gov/pub/station/general/igs.snx

 - For VLBI solutions you can use

   http://gemini.gsfc.nasa.gov/solve_save/ECCDAT.ecc

 - The official ILRS eccentricity files (in SINEX format) are

   ftp://cddisa.gsfc.nasa.gov/pub/slrocc/ecc_une.snx

       for eccentricities in Up, North, East

   and

   ftp://cddisa.gsfc.nasa.gov/pub/slrocc/ecc_xyz.snx

       for eccentricities in X, Y, Z

18. SOLUTION/EPOCHS Block (Mandatory)

 Description:

 List of solution epoch for each Site Code/Point Code/Solution 

Number/Observation Code (SPNO) combination.

 Contents:


 ___________________________________________________________________


|____S_O_L_U_T_I_O_N___E_P_O_C_H_S___D_A_T_A___L_I_N_E______________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Site Code]    | Site code for which some          |   1X,A4      |


|                | parameters are estimated.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point Code at a site for which    |   1X,A2      |


|                | some parameters are estimated.    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution Number at a Site/Point   |   1X,A4      |


|                | code for which some parameters    |              |


|                | are estimated.                    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Observation   | Identification of the observation |   1X,A1      |


| Code]          | technique used.                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Start time for which the solution |   1X,I2.2,   |


|                | identified (SPNO) has observations|   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | End time for which the solution   |   1X,I2.2,   |


|                | identified (SPNO) has observations|   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Mean time of the observations for |   1X,I2.2,   |


|                | which the solution (SPNO) is      |   1H:,I3.3,  |


|                | derived.                          |   1H:,I5.5   |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     54       |

                                                           |______________|

19. BIAS/EPOCHS Block (Mandatory if bias parameters are included)

 Description:

 List of epochs of bias parameters for each Site Code/Point Code/Solution 

Number/Bias Type (SPNB) combination for which a bias parameter is solved.

 Contents:  


 ___________________________________________________________________


|______________B_I_A_S___E_P_O_C_H_S___D_A_T_A___L_I_N_E____________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| [Site Code]    | Site code for which some biases   |   1X,A4      |


|                | are estimated (station ID)        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | satellite ID for which some biases|   1X,A2      |


|                | are estimated:                    |              |

      |                | e.g. L1, L2 for LAGEOS-1 and -2   |              |

      |                |      respectivly                  |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | sequential number of the bias for |   1X,A4      |


|                | this particular station           |              |


|                | (if just one bias is solved for a |              |

      |                | particular station, this parameter|              |

      |                | remains "1").                     |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Bias Type      | Specification of the type of bias:|   1X,A1      |


|                | R - range bias                    |              |

      |                | T - time bias                     |              |

      |                | S - scale bias                    |              |

      |                | Z - troposphere bias at zenith    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Epoch of 1st observation of the   |   1X,I2.2,   |


|                | solution identified (SPNB)        |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Epoch of last observation of the  |   1X,I2.2,   |


|                | solution identified (SPNB)        |   1H:,I3.3,  |


|                |                                   |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Weighted mean time of the         |   1X,I2.2,   |

      |                | observations for which the        |   1H:,I3.3,  |


|                | solution (SPNB) is derived.       |   1H:,I5.5   |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     54       |

                                                           |______________|

20. SOLUTION/STATISTICS Block (Recommended if available)

 Description:

 Statistical information about the solution contained in the SINEX file.

 Contents:

 
 ___________________________________________________________________


|____S_O_L_U_T_I_O_N___S_T_A_T_I_S_T_I_C_S_____L_I_N_E______________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Information    | Describes the type of information |   1X,A30     |


| Type           | present in the next field. May    |              |


|                | take on the following values:     |              |


|                |                                   |              |


|                |'NUMBER OF OBSERVATIONS'           |              |


|                |   # of observations used in the   |              |


|                |   adjustment.                     |              |


|                |'NUMBER OF UNKNOWNS'               |              |


|                |   # of unknowns solved in the     |              |


|                |   adjustment.                     |              |


|                |'SAMPLING INTERVAL (SECONDS)'      |              |


|                |   Interval in seconds between     |              |


|                |   successives observations.       |              |


|                |'SQUARE SUM OF RESIDUALS (VTPV)'   |              |


|                |   Sum of squares of residuals.    |              |

      |                |   (V'PV); V - resid. vector;      |              |

      |                |           P - weight matrix       |              |


|                |'PHASE MEASUREMENTS SIGMA'         |              |


|                |   Sigma used for the phase        |              |


|                |   measurements.                   |              |


|                |'CODE MEASUREMENTS SIGMA'          |              |


|                |   Sigma used for the code (pseudo-|              |


|                |   range) measurements.            |              |


|                |'NUMBER OF DEGREES OF FREEDOM'     |              |


|                |    # of observations minus the    |              |


|                |    # of unknowns                  |              |

      |                |    (df)                           |              |


|                |'VARIANCE FACTOR'                  |              |


|                |    Sum of squares of residuals    |              |


|                |    divided by the degrees of      |              |


|                |    freedom (V'PV/df). Equivalent  |              |

      |                |    to  Chi-squared/df.            |              |

      |                |'WEIGHTED SQUARE SUM OF O-C'       |              |

      |                |    Sum of squares of the vector   |              |

      |                |    'observed minus computed':     |              |

      |                |    (o-c)'P(o-c)                   |              |

      |                |    with P - weigth matrix         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Information    | Relevant information for the type |   1X,F22.15  |


|                | indicated by the previous field.  |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     54       |

                                                           |______________|

 Comments:

 The mentioned 'Information Types' may be in any order but the name of the fields should be identical to the names listed above.

 Note that the NUMBER OF UNKNOWNS contains all parameters of the adjustment, i.e., not only the parameters stored in the SINEX file but as well all the pre-eliminated parameters.

 The NUMBER OF OBSERVATIONS should contain only the real observations and not the pseudo-observations used for constraining.

 In principle the estimated variance-covariance matrix should be normalized / multiplied by the VARIANCE FACTOR of this statistic block.

21. SOLUTION/ESTIMATE Block (Mandatory)

 Description:

 Estimated parameters.

 Contents:  


 ___________________________________________________________________


|______S_O_L_U_T_I_O_N___E_S_T_I_M_A_T_E___D_A_T_A___L_I_N_E________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Estimated Para-| Index of estimated parameters.    |   1X,I5      |


| meters Index   | values from 1 to the number of    |              |


|                | parameters.                       |              |


|________________|___________________________________|______________|


|                |                                   |              |


|[Parameter Type]| Identification of the type of     |   1X,A6      |


|                | parameter.                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Site Code]    | Site code for which some          |   1X,A4      |


|                | parameters are estimated.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point Code at a site or the       |   1X,A2      |

      |                | satellite ID for which some       |              |


|                | parameters are estimated.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution ID at a Site/Point       |   1X,A4      |


|                | code for which some parameters    |              |


|                | are estimated.                    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Epoch at which the estimated      |   1X,I2.2,   |


|                | parameter is valid.               |   1H:,I3.3,  |


|                | For bias parameters the beginning |   1H:,I5.5   |

      |                | of the pass (identical to the     |              |

      |                | BIAS/EPOCHS block).               |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Parameter Units| Units used for the estimates and  |   1X,A4      |


|                | sigmas. The notations are:        |              |


|                | m    (metres),                    |              |

      |                | m/y  (metres per year),           |              |

      |                | m/s2 (metres per second**2),      |              |

      |                | ppb  (parts per billion),         |              |


|                | ms   (milliseconds),              |              |

      |                | msd2 (milliseconds per day**2),   |              |


|                | mas  (milli-arc-seconds),         |              |

      |                | ma/d (milli-arc-seconds / day),   |              |

      |                | rad  (radians),                   |              |

      |                | rd/y (radians per year),          |              |

      |                | rd/d (radians per day).           |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Constraint    | Constraint applied to the parame- |   1X,A1      |


| Code]          | ter.                              |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Parameter      | Estimated value of the parameter. |   1X,E21.15  |


| Estimate       |                                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Parameter      | Estimated standard deviation for  |   1X,E11.6   |


| Standard       | the parameter.                    |              |


| Deviation      |                                   |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

 Comments:

 For the demanded units of the estimated parameters and their standard deviation please refer to the list of possible parameter types (2. Data Structure).

 'Per year' means 365.25 days in this context. 

22. SOLUTION/APRIORI Block (Mandatory)

 Description:

 Apriori information for estimated parameters, either the used apriori values for the adjustment or the parameters of a Helmert Transformation for applied inner constraints with the constraint given in the field 'Standard Deviation'. 

 Contents:


 ___________________________________________________________________


|________S_O_L_U_T_I_O_N___A_P_R_I_O_R_I___D_A_T_A___L_I_N_E________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Parameter      | Index of apriori parameters.      |   1X,I5      |


| Index          |                                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


|[Parameter Type]| Identification of the type of     |   1X,A6      |

      |                | parameter.                        |              |

      |                | For apriori values of estimated   |              |

      |                | parameters see parameter list     |              |

      |                | above;                            |              |


|                | For inner constraints:            |              |

      |                | TX - Translation in X-direction  m|              |

      |                | TY - Translation in Y-direction  m|              |

      |                | TZ - Translation in Z-direction  m|              |

      |                | RX - Rotation around X-axis    mas|              |

      |                | RY - Rotation around Y-axis    mas|              |

      |                | RZ - Rotation around Z-axis    mas|              |

      |                | SC - Scale                     ppb|              |

      |                | TXR – Rate for translation in     |              |

      |                |       X-direction              m/y|              |

      |                | TYR – Rate for translation in     |              |

      |                |       Y-direction              m/y|              |

      |                | TZR – Rate for translation in     |              |

      |                |       Z-direction              m/y|              |

      |                | RXR – Rate for rotation around    |              |

      |                |       X-axis                 mas/y|              |

      |                | RYR – Rate for rotation around    |              |

      |                |       Y-axis                 mas/y|              |

      |                | RZR – Rate for rotation around    |              |

      |                |       Z-axis                 mas/y|              |

      |                | SCR – Rate for scale         ppb/y|              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Site Code]    | Site code with apriori parameter  |   1X,A4      |


|                | estimate.                         |              |

      |                | ---- for inner constraints        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point Code with apriori parameter |   1X,A2      |


|                | estimate.                         |              |

      |                | -- for inner constraints          |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution ID at a Site/Point       |   1X,A4      |


|                | code with apriori parameter       |              |


|                | estimate.                         |              |

      |                | ---- for inner constraints        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Epoch at which the apriori        |   1X,I2.2,   |


|                | parameter or the inner constraint |   1H:,I3.3,  |

      |                | is valid.                         |   1H:,I5.5   |


|________________|___________________________________|______________|


|                |                                   |              |


| Parameter Units| Units used for the aprioris and   |   1X,A4      |


|                | sigmas. For the demanded units    |              |


|                | look at SOLUTION/ESTIMATE block.  |              |


|                | For the inner constraints the     |              |

      |                | units should be:                  |              |

      |                | m    for translations,            |              |

      |                | mas  for rotations,               |              |

      |                | ppb  for scale,                   |              |

      |                | m/y  for translation rates,       |              |

      |                | ma/y for rotation rates,          |              |

      |                | pb/y for scale rates              |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Constraint    | Constraint applied to the parame- |   1X,A1      |


| Code]          | ter.                              |              |

      |                | If inner constraints are applied: |              |

      |                | 1 for contributing stations       |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Parameter      | Apriori value of the parameter or |   1X,E21.15  |


| Apriori        | transformation parameter for the  |              |

      |                | inner constraint.                 |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Parameter      | Apriori standard deviation for    |   1X,E11.6   |


| Standard       | the parameter or applied inner    |              |

      | Deviation      | constraint.                       |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     80       |

                                                           |______________|

 Comments:

 If inner constraints are applied to the solution (i.e. parameters like TX, TY, TZ, RX,... are included) the stations contributing to these inner constraints should be listed with a '1' in the field 'Constraint Code' in this SOLUTION/APRIORI block.

23. SOLUTION/MATRIX_ESTIMATE Block (Mandatory)

 Description:

 The Estimate Matrix can be stored in an Upper or Lower triangular form. Only

the Upper or Lower portion needs to be stored because the matrix is always

symmetrical.

 The matrix contents can be:

CORR
- Correlation Matrix

COVA
- Covariance Matrix

INFO
- Information Matrix (of Normals), i.e. COVA^(-1)

The distinction between the form and its contents is given by the title block

which must take one of the following forms:

 SOLUTION/MATRIX_ESTIMATE L CORR

 SOLUTION/MATRIX_ESTIMATE U CORR

 SOLUTION/MATRIX_ESTIMATE L COVA

 SOLUTION/MATRIX_ESTIMATE U COVA

 SOLUTION/MATRIX_ESTIMATE L INFO

 SOLUTION/MATRIX_ESTIMATE U INFO

 Contents: 


 ___________________________________________________________________


|S_O_L_U_T_I_O_N__M_A_T_R_I_X__E_S_T_I_M_A_T_E____D_A_T_A___L_I_N_E_|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Matrix Estimate| Row index for the Matrix Estimate.|   1X,I5      |


| Row Number     | It must match the parameter index |              |


|                | in the SOLUTION/ESTIMATE block    |              |


|                | for the same parameter.           |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Matrix Estimate| Column index for the Matrix Esti- |   1X,I5      |


| Column Number  | mate. It must match the parameter |              |


|                | index in the SOLUTION/ESTIMATE    |              |


|                | block for the same parameter.     |              |


|________________|___________________________________|______________|


|                |                                   |              |


| First Matrix   | Matrix element at the location    |   1X,E21.14  |


|Estimate Element| ( Row Number , Column Number ).   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Second Matrix  | Matrix element at the location    |   1X,E21.14  |


|Estimate Element| ( Row Number , Column Number + 1).|              |


|________________|___________________________________|______________|


|                |                                   |              |


| Third  Matrix  | Matrix element at the location    |   1X,E21.14  |


|Estimate Element| ( Row Number , Column Number + 2).|              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     78       |

                                                           |______________|

 Comment:

 The Matrix Estimate Row/Column Number correspond to the Estimated Parameters 

Index in the SOLUTION/ESTIMATE block.

 If the CORR matrix is used, standard deviations must be stored in the diagonal elements instead of 1.000.

 Missing elements in the matrix are assumed to be zero (0); consequently, zero

elements may be omitted to reduce the size of this block. 

 NOTE: The same scale (variance) factor MUST be used for both MATRIX_ESTIMATE

and MATRIX_APRIORI, as well as for the standard deviations in the ESTIMATE

and APRIORI Blocks. This scale factor should be stored as 'Variance Factor' in the SOLUTION/STATISTICS block.

 If you use the INFO type this block should contain the constrained normal equation matrix of your least square adjustment.

24. SOLUTION/MATRIX_APRIORI Block (Recommended/Mandatory)

 Description:

 The Apriori Matrix can be stored in an Upper or Lower triangular form. Only

the Upper or Lower portion needs to be stored because the matrix is always

symmetrical. Mandatory if any significant constraint have been applied to the 

SOLUTION/ESTIMATE.

 The matrix contents can be:

CORR
- Correlation Matrix

COVA
- Covariance Matrix

INFO
- Information Matrix (of Normals), i.e. COVA^(-1)

The distinction between the form and its contents is given by the title block

which must take one of the following forms:

 SOLUTION/MATRIX_APRIORI L CORR

 SOLUTION/MATRIX_APRIORI U CORR

 SOLUTION/MATRIX_APRIORI L COVA

 SOLUTION/MATRIX_APRIORI U COVA

 SOLUTION/MATRIX_APRIORI L INFO

 SOLUTION/MATRIX_APRIORI U INFO

 Contents: 


 ___________________________________________________________________


|__S_O_L_U_T_I_O_N__M_A_T_R_I_X__A_P_R_I_O_R_I____D_A_T_A___L_I_N_E_|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Matrix Apriori | Row index for the Matrix Apriori. |   1X,I5      |


| Row Number     | It must match the parameter index |              |


|                | in the SOLUTION/APRIORI block     |              |


|                | for the same parameter.           |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Matrix Apriori | Column index for the Matrix       |   1X,I5      |


| Column Number  | Apriori. It must match the        |              |


|                | parameter index in the            |              |


|                | SOLUTION/APRIORI block for the    |              |

      |                | same parameter.                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| First Matrix   | Matrix element at the location    |   1X,E21.16  |


|Estimate Element| ( Row Number , Column Number ).   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Second Matrix  | Matrix element at the location    |   1X,E21.16  |


|Estimate Element| ( Row Number , Column Number + 1).|              |


|________________|___________________________________|______________|


|                |                                   |              |


| Third  Matrix  | Matrix element at the location    |   1X,E21.16  |


|Estimate Element| ( Row Number , Column Number + 2).|              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     78       |

                                                           |______________|

 Comment:

 The Matrix Apriori Row/Column Number correspond to the Apriori Parameters Index

in the SOLUTION/APRIORI block. If the apriori constraint matrix is diagonal and

no loss of significant digits occurs by using the Parameter Standard Deviation

in the SOLUTION/APRIORI block, then, this block becomes redundant.

 If the CORR matrix is used, Standard deviations must be stored in the diagonal elements instead of 1.000.

 Missing elements in the matrix are assumed to be zero (0); consequently, zero

elements may be omitted to reduce the size of this block. 

 NOTE: The same scale (variance) factor MUST be used for both MATRIX_ESTIMATE

and MATRIX_APRIORI, as well as for the standard deviations in the ESTIMATE

and APRIORI Blocks. This scale factor should be stored as 'Variance Factor' in the SOLUTION/STATISTICS block.

 If you use the INFO type this block should contain the normal equation matrix of the constraints applied to your solution in SOLUTION/ESTIMATE.

25. SOLUTION/NORMAL_EQUATION_VECTOR Block (Mandatory for normal equations)

 Description:

 If the SINEX file shall provide the normal equation directly this block is mandatory and contains the vector of the right hand side of the unconstrained (reduced) normal equation.

 Contents:


 ___________________________________________________________________

      |_SOLUTION__N_O_R_M_A_L___E_Q_U_A_T_I_O_N___V_E_C_T_O_R___DATA_LINE_|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| Estimated Para-| Index of estimated parameters.    |   1X,I5      |


| meters Index   | Values from 1 to the number of    |              |


|                | parameters. It must match the     |              |

      |                | parameter index in the block      |              |

      |                | SOLUTION/ESTIMATE for the same    |              |

      |                | parameter.                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


|[Parameter Type]| Identification of the type of     |   1X,A6      |


|                | parameter.                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Site Code]    | Site code for which some          |   1X,A4      |


|                | parameters are estimated.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Point Code]   | Point Code at a site or the       |   1X,A2      |

      |                | satellite ID for which some       |              |


|                | parameters are estimated.         |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Solution ID]  | Solution ID at a Site/Point       |   1X,A4      |


|                | code for which some parameters    |              |


|                | are estimated.                    |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Time]         | Epoch at which the estimated      |   1X,I2.2,   |


|                | parameter is valid.               |   1H:,I3.3,  |


|                | For bias parameters the beginning |   1H:,I5.5   |

      |                | of the pass (identical to the     |              |

      |                | BIAS/EPOCHS block).               |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Parameter Units| see SOLUTION/ESTIMATE             |   1X,A4      |


|                |                                   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| [Constraint    | Constraint applied to the parame- |   1X,A1      |


| Code]          | ter.                              |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Right hand     | Value of the right hand side of   |   1X,E21.15  |


| side of normal | the normal equation for the       |              |

      | equation       | corresponding parameter.          |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     68       |

                                                           |______________|

 Comment:

 The indices correspond to the indices of the SOLUTION/ESTIMATE block.

26. SOLUTION/NORMAL_EQUATION_MATRIX Block (Mandatory for normal equations)

 Description:

 This block is mandatory if the normal equation is to be provided directly in the SINEX file.

 The block should contain the original (reduced) normal equation matrix (i.e., without constraints).

 The normal equation matrix can be stored in an Upper or Lower triangular form. Only the Upper or Lower portion needs to be stored because the matrix is always

symmetrical. The distinction between the forms is given by the title block

which must take one of the following forms:

 SOLUTION/NORMAL_EQUATION_MATRIX L 

 SOLUTION/NORMAL_EQUATION_MATRIX U

 Contents:

 
 ___________________________________________________________________

      |_SOLUTION__N_O_R_M_A_L___E_Q_U_A_T_I_O_N___M_A_T_R_I_X___DATA_LINE_|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| NEQ-Matrix     | Row index for the normal equation |   1X,I5      |


| Row Number     | matrix. It must match the         |              |


|                | parameter index in the SOLUTION/  |              |


|                | ESTIMATE block for the same       |              |

      |                | parameter.                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| NEQ-Matrix     | Column index for the normal       |   1X,I5      |


| Column Number  | equation matrix. It must match the|              |


|                | parameter index in the SOLUTION/  |              |


|                | ESTIMATE block for the same       |              |

      |                | parameter.                        |              |


|________________|___________________________________|______________|


|                |                                   |              |


| First Matrix   | Matrix element at the location    |   1X,E21.14  |


| Element        | ( Row Number , Column Number ).   |              |


|________________|___________________________________|______________|


|                |                                   |              |


| Second Matrix  | Matrix element at the location    |   1X,E21.14  |


| Element        | ( Row Number , Column Number + 1).|              |


|________________|___________________________________|______________|


|                |                                   |              |


| Third  Matrix  | Matrix element at the location    |   1X,E21.14  |


| Element        | ( Row Number , Column Number + 2).|              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |     78       |

                                                           |______________|

 Comment:

 The NEQ-Matrix Row/Column Number correspond to the Estimated Parameters 

Index in the SOLUTION/ESTIMATE block.

 Missing elements in the matrix are assumed to be zero (0); consequently, zero

elements may be omitted to reduce the size of this block. 

27. Footer Line  (Mandatory)

 Description:

 Marks the end of the SINEX file.

 Contents:  

        ___________________________________________________________________


|_____________F_O_O_T_E_R___L_I_N_E_________________________________|


|                |                                   |              |


|__Field_________|______Description__________________|___Format_____|


|                |                                   |              |


| End of SINEX   | The seven characters %ENDSNX at   |   A7         |

      |                | the beginning of the last line    |              |

      |                | mark the end of the SINEX file.   |              |


|________________|___________________________________|______________|

                                                           |              |

                                                           |      7       |

                                                           |______________|

-------------------------------------------------------------------------------------
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          A P P E N D I X   II

                S U M M A R Y   O F   F O R M U L A S   A N D

              T H E I R   C O N N E C T I O N   T O   S I N E X

This document gives a short summary of the basic formulas used for least squares adjustment and it gives instructions which vector or matrix of the normal equation system belongs to the individual SINEX blocks.

 SUMMARY OF LEAST SQUARES ADJUSTMENT FORMULAS

You have n_obs linearized observation equations

(1)   v  =  A dx  -  l

where

 n_obs  number of observations

 v      residual vector

 A      Jacobian matrix

 dx     corrections for the unknowns x concerning the apriori values x0

        i.e. x = x0 + dx 

with

 n_unk  number of unknowns

 l      vector 'observed' minus 'computed with apriori values'.

 P      denotes the weight matrix for the observations.

The goal of least square adjustment is to minimize the square sum of residuals:

(2)   v' P v  =  min

where v' is the transposed vector of v.

This condition leads to the so called normal equation

(3) A' P A dx  =  A' P l

with normal equation matrix

(4) N  =  A' P A

and the vector of the right hand side of the normal equation

(5) b  =  A' P l .

The resulting unknown parameters can be determined with

(6) x  =  x0  +  inv(A' P A) A' P l  =  x0  +  inv(N) b

where inv stands for the inverse matrix and x0 are the apriori values.

The residuals can be computed with equation (1) and the aposteriori variance factor is then

(7) s0  =  (v' P v) / (n_obs - n_unk) .

The weighted square sum o fthe vector l (= observed minus computed) can be obtained with

(8) l’Pl = v’Pv  +  dx’ b

         = v’Pv  +  dx’ A’ P l .

The variance-covariance matrix of the unknowns results in

(9) K  =  s0 inv(N).

If you introduce constraints as pseudo-observations with n_constr linearized observation equations

(10) v_c  =  H dx  -  h

with

 n_constr  number of constraints as pseudo-observations

 v_c       residuals over the constraints

 H         Jacobian matrix for pseudo-observation equations

 h         vector 'observed' minus 'computed' for the constraints.

P_c denotes the weight matrix for your pseudo-observations.

The least square methods lead to the normal equation for the pseudo-observations

(11) H' P_c H dx  =  H' P_c h

with normal equation matrix of constraints

(12) N_constr  =  H' P_c H

and vector of the right hand side of normal equation for constraints

(13) b_constr  =  H' P_c h.

The complete normal equation system for the constrained solution can easily be computed:

(14) (A' P A  +  H' P_c H) dx  =  A' P l  +  H' P_c h

with the constrained normal equation matrix

(15) N_total  =  A' P A  +  H' P_c H  =  N  +  N_constr

and the vector of the right hand side of the constrained normal equation system

(16) b_total  =  A' P l  +  H' P_c h  =  b  +  b_constr .

The unknown parameters of the constrained solution can be computed with

(17) x_c  =  x0  +  inv(N_total) b_total .

Ater computing the residuals over the constraints with equation (10) the weighted square sum of residuals of the constrained normal equation system can be obtained with

(18) v’Pv + v_c’ P_c v_c 

and the number of degrees of freedom of the constrained normal equation system is

(19) dof = n_obs + n_constr – n_unk .

The aposteriori variance-factor for the constrained normal equation system is then

(20) s0_c  =  (v' P v  +  v_c' P_c v_c) / dof .

The variance-covariance matrix for the unknowns of this constrained normal equation system can be computed with

(21) K_xx  =  s0_c  inv(N_total)

And the variance-covariance matrix for the constraints is

(22) K_constr  =  s0_c  inv(N_constr) .

 IMPLEMENTATION IN SINEX

The different elements belonging to the normal equations can be stored in SINEX files in the following way:

SOLUTION/STATISTICS block:

      n_unk                     = NUMBER OF UNKNOWNS

      n_obs                     = NUMBER OF OBSERVATIONS

 (20) s0_c                      = VARIANCE FACTOR

 (18) v' P v + v_c' P_c v_c     = SQUARE SUM OF RESIDUALS (VTPV)

 (19) dof                       = NUMBER OF DEGREES OF FREEDOM

SOLUTION/ESTIMATE block:

 (17) x_c    in field "Parameter Estimate"

SOLUTION/APRIORI block:

      x0  in field "Parameter Apriori"

SOLUTION/MATRIX_ESTIMATE block:

 (21) Type COVA:  K_xx

      Type CORR:  correlation matrix of K_xx

 (15) Type INFO:  N_total  =  N + N_constr

SOLUTION/MATRIX_APRIORI block:

 (22) Type COVA:  K_constr

      Type CORR:  correlation matrix of K_constr

 (12) Type INFO:  N_constr

SOLUTION/NORMAL_EQUATION_VECTOR block:

 (5)  b  =  A' P l

SOLUTION/NORMAL_EQUATION_MATRIX block:

 (4)  N  =  A' P A 

